>> MIB - Management Information Base
>> Table: dot11PhyOFDMTable - (.1.2.840.10036.4.11.1)
Description: An entry in the dot11PhyOFDM Table. ifIndex - Each IEEE 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11PhyOFDMTable
OID | Name | Type | Access
.1 | CurrentFrequency | INTEGER | RW
.2 | TIThreshold | Integer32 | RW
.3 | FrequencyBandsSupported | INTEGER | R
CurrentFrequency
The number of the current operating frequency channel of the OFDM PHY. Range: 0 to 255
TIThreshold
The Threshold being used to detect a busy medium (frequency). CCA shall report a busy medium upon detecting the RSSI above this threshold.
FrequencyBandsSupported
The capability of the OFDM PHY implementation to operate in the three U-NII bands. Coded as an integer value of a three bit field as follows: bit 0 .. capable of operating in the lower (5.15-5.25 GHz) U-NII band bit 1 .. capable of operating in the middle (5.25-5.35 GHz) U-NII band bit 2 .. capable of operating in the upper (5.725-5.825 GHz) U-NII band For example, for an implementation capable of operating in the lower and mid bands this attribute would take the value 3. Range: 1 to 7

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH