>> MIB - Management Information Base
>> Table: mpsWaveFileTable - (.1.3.6.1.4.1.272.4.53.13.4.1)
Description: This entry only is created by the respective device driver
mpsWaveFileTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Description | DisplayString | RW
.3 | Directory | DisplayString | RW
.4 | Name | DisplayString | RW
.5 | AcousticProperties | DisplayString | R
.6 | Size | INTEGER | RW
.7 | Duration | INTEGER | R
.8 | Volume | INTEGER | RW
.9 | Status | ENUM | RW
.10 | UploadResult | ENUM | RW
Index
A unique index for each wave file table entry. Range: 1 to 255
Description
The description can be used to assign an alias name to the wave file. Length: 0 to 32
Directory
Specifies the complete path/tree where the wave file can be found on the mounted device. Length: 0 to 255
Name
Simply contains the wave file name on the mounted device. Length: 0 to 255
AcousticProperties
Optionally contains acoustic properties of the wave file: e.g. audioformat, bit-rate, sample-rate etc. Length: 0 to 255
Size
This variable contains the wave file size in kbytes.
Duration
This variable contains the wave file (music) duration in seconds.
Volume
This variable contains the volume adjustment level for the wave file to be played back with (approximately in 3 dB steps): negative values -> attenuate during playback 0 -> playback as recorded (default) positive values -> amplify during playback Range: -5 to 3
Status
Wave file status: create(1) -> new wave file shall be stored on the device remove(2) -> wave file shall be deleted on the storage device done(3) -> synchronization of storage device with MIB is done. Enumerations: create (1) remove (2) done (3)
UploadResult
Wave file upload result (error) code: success(1) -> the wave file upload was successful, no-mem-card(2) -> no memory card plugged, no-mem-space(3) -> no more space available on the memory card, incomp-wav-format(4) -> the wave file format doesn't match the requirements, transfer-error(5) -> any transfer error occured during upload. Enumerations: success (1) no-mem-card (2) no-mem-space (3) incomp-wav-format (4) transfer-error (5) write-protection (6)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH