>> MIB - Management Information Base
>> Table: biboPPPLinkTable - (.1.3.6.1.4.1.272.4.3.3.1)
Description: The biboPPPLinkTable contains statistical information for each current PPP link on the system. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new PPP interface is created in the biboPPPTable. Deleting entries: Entries are removed by the system when the corresponding PPP interface is removed.
biboPPPLinkTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Established | Date | R
.3 | Direction | ENUM | R
.4 | Protocols | INTEGER | R
.5 | State | ENUM | R
.6 | Units | Counter | R
.7 | Retries | Counter | R
.8 | KeepaliveSent | Counter | R
.9 | KeepalivePending | Counter | R
.10 | DeviceIndex | INTEGER | R
.11 | Speed | INTEGER | R
.13 | StkNumber | INTEGER | R
.14 | CallType | ENUM | R
.15 | CallReference | INTEGER | R
.16 | Charge | Counter | R
.17 | Accm | OCTET STRING | R
.18 | Lqm | ENUM | R
.19 | LcpComp | ENUM | R
.20 | LocDiscr | OCTET STRING | R
.21 | RemDiscr | OCTET STRING | R
.22 | L1Protocol | ENUM | R
.23 | LocAuth | ENUM | R
.24 | RemAuth | ENUM | R
.25 | NRxDesc | INTEGER | R
.26 | NTxDesc | INTEGER | R
IfIndex
Correlating PPP interface index.
Established
Time when the link was established. Range: 0 to -1
Direction
Direction of link, incoming(1) or outgoing(2). In case of permanent links, the meaning is dce(1) or dte(2). Enumerations: incoming-dce (1) outgoing-dte (2)
Protocols
The bitwise ORed protocols successfully negotiated on this link; currently the following protocols are supported: tcp/ip(1), ipx(2), bridge(4), bpdu(8), x25(16). These protocol values are most likely to change in future software releases.
State
The actual state of each link in a bundle. The link is fully operational in the up(1) state, and not operational in the down(2) state. The starting(3) state is an inter- mediate state when the link is physically established but PPP or other link negotation has not finished yet. The loopbacked(4) state is entered when the PPP keepalive mechanism detects a loopbacked link. The dialing(5) state shows that a dialup link is in its link establishment phase, dialing. If there is no answer to the call, the link enters the retry-wait(6) state for biboPPPRetryTime seconds. After waiting that time either a call retry will occur, or the ifOperStatus will enter the blocked state, depending on the amount of retries already done (biboPPPLinkRetries) and the value of the biboPPPMaxRetries field. Enumerations: up (1) down (2) starting (3) loopbacked (4) dialing (5) retry-wait (6)
Units
The costs for this link in units.
Retries
The amount of retries taken to establish the link.
KeepaliveSent
The amount of keepalive packets sent on the link.
KeepalivePending
The amount of keepalive answer packets waiting for since the last occurance of an echo reply packet.
DeviceIndex
The underlying link device index.
Speed
The speed of the link.
StkNumber
The stack number of the dialup link, correlating to the isdnCallStkNumber field in the isdnCallTable. Range: 0 to 31
CallType
The call type of the dialup link, correlating to the isdnCallType field in the isdnCallTable. Enumerations: incoming (1) outgoing (2) undef (3)
CallReference
The call reference of the dialup link, correlating to the isdnCallReference field in the isdnCallTable.
Charge
The costs for this link as 1/1000 of the respective currency.
Accm
The Asynchronous Control Character Map (ACCM) according RFC 1662. Length: 4 to 4
Lqm
Indicates the successful negotiation of the Link Quality Protocol (LQM). Enumerations: none (1) negotiated (2)
LcpComp
Address- and Protocol-Field compression. Enumerations: none (1) addr (2) prot (3) both (4)
LocDiscr
Local LCP multilink endpoint discriminator. Length: 6 to 6
RemDiscr
Peer's LCP multilink endpoint discriminator. Length: 20 to 20
L1Protocol
The layer 1 protocol of this link. Enumerations: data-64k (1) data-56k (2) modem (3) dovb (4) v110-1200 (5) v110-2400 (6) v110-4800 (7) v110-9600 (8) v110-14400 (9) v110-19200 (10) v110-38400 (11) modem-profile-1 (12) modem-profile-2 (13) modem-profile-3 (14) modem-profile-4 (15) modem-profile-5 (16) modem-profile-6 (17) modem-profile-7 (18) modem-profile-8 (19) pptp-pns (20) pppoe (21) pppox25 (22) pptp-pac (23) pppoa (24) l2tp-lns (25) l2tp-lac (26) dovb-64k (28)
LocAuth
The result of the PPP authentication procedure performed locally. Enumerations: none (1) successful (2) failed (3) timeout (4) prot-rejected (5)
RemAuth
The result of the PPP authentication procedure performed on remote. Enumerations: none (1) successful (2) failed (3) timeout (4) prot-rejected (5)
NRxDesc
This variable contains the number of receive descriptors used by the interface driver of the respective link. Range: 0 to 2048
NTxDesc
This variable contains the number of transmit descriptors used by the interface driver of the respective link. Range: 0 to 2048

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH