>> MIB - Management Information Base
>> Table: upnpGlobals - (.1.3.6.1.4.1.272.4.5.45.10)
upnpGlobals
OID | Name | Type | Access
.10 | Status | ENUM | RW
.20 | TcpPort | INTEGER | RW
.30 | SsdpTtl | INTEGER | RW
Status
This object specifies whether UPnP is enabled on the router. Possible values: enabled(10), -- UPnP enabled restricted(20), -- UPnP mapping requests for client IP only disabled(30) -- UPnP disabled (default). Enumerations: enabled (10) restricted (20) disabled (30)
TcpPort
The TCP port which is monitored by UPnP for HTTP requests received from UPnP clients. Range: 1 to 65535
SsdpTtl
The time-to-live value for SSDP packet transmitted on the LAN. If this object is set to 0, the default value specified in the ip MIB will be used instead. Range: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH