>> MIB - Management Information Base
>> Table: ip6LinkPrefixTable - (.1.3.6.1.4.1.272.4.5.100.1.6.1)
Description: A link prefix entry.
ip6LinkPrefixTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | RW
.2 | PrefixId | INTEGER | RW
.3 | AdminStatus | ENUM | D
.4 | SiteLevelValue | Unsigned32 | RW
.5 | Length | INTEGER | RW
.6 | OnLinkFlag | ENUM | RW
.7 | AutonomousFlag | ENUM | RW
.8 | AdvValidLifetime | Unsigned32 | RW
.9 | AdvPreferredLifetime | Unsigned32 | RW
.10 | Prefix | InetAddressIPv6 | R
.11 | OperStatus | ENUM | R
.12 | Id | INTEGER | RW
.13 | Slaac | ENUM | RW
.14 | Advertise | ENUM | RW
.15 | Descr | DisplayString | RW
.16 | AdmPrefix | InetAddressIPv6 | RW
.17 | DhcpOptionSetId | INTEGER | RW
.18 | OpValidLifetime | Unsigned32 | R
.19 | OpPreferredLifetime | Unsigned32 | R
IfIndex
Interface on which the prefix will published. Range: 1 to 2147483647
PrefixId
Ident of the associated administrative prefix, see ip6AdmPrefixEntryTable.
AdminStatus
Administrative status of this entry. Enumerations: enable (1) disable (2) delete (3)
SiteLevelValue
SiteLevel Identifier SLA.
Length
The Length of the new generated prefix, Range: 48 to 64
OnLinkFlag
true: prefix can be used for on-link determination Enumerations: true (1) false (2)
AutonomousFlag
Determines whether the Autonomous address configuration flag within the Router Advertisement Message (RFC 4861) should be set or not. true: set the flag - stateless configuration possible false: don't set the flag - no autoconfiguration possible Enumerations: true (1) false (2)
AdvValidLifetime
Configured maximum 'valid lifetime'. More details are described for field 'ip6LinkPrefixOpValidLifetime'.
AdvPreferredLifetime
Configured maximum 'prefered lifetime'. More details are described for field 'ip6LinkPrefixOpPreferredLifetime'.
Prefix
The current used prefix for this link. Length: 16 to 16
OperStatus
The operational status. Enumerations: up (1) down (2)
Id
Unique ID of this table-entry.
Slaac
SLAAC method, this setting determines the address format which should be the result of the address autoconfiguration procedure eui64 EUI-64-Identifier according RFC 4291 privacy-ext Privacy Extensions according RFC 4941 disabled no SLAAC Enumerations: eui64 (1) disabled (3)
Advertise
Specifies the propagation policy for this entry when sending a Router Advertisement (RA) via the associated interface enabled include prefix in RA disabled ignore this prefix when sending RA's Enumerations: enabled (1) disabled (2)
Descr
User defined description of this link prefix entry Length: 0 to 255
AdmPrefix
The configured prefix for this link - without any reference to a general prefix. Length: 16 to 16
DhcpOptionSetId
If not set to 0 and if 'ip6DhcpOptionSet' entry with matching 'Id' value exists then internal DHCPv6-server uses this prefix for building requested IA_NA options (see 22.4 and 22.6 of RFC-3315). In this case, 'ip6LinkPrefixOnLinkFlag' must be set to 'true' and 'ip6LinkPrefixAutonomousFlag' must be set to 'false' for proper configuration. Range: 0 to 65535
OpValidLifetime
'Operative' valid lifetime. If 'ip6LinkPrefixPrefixId' does NOT refer to valid 'ip6Prefix' then lifetime is set to configured 'ip6LinkPrefixAdvValidLifetime'. Otherwise, it is set to minimum of configured value and inherited 'ip6PrefixAdvValidLifetime'.
OpPreferredLifetime
'Operative' preferred lifetime. If 'ip6LinkPrefixPrefixId' does NOT refer to valid 'ip6Prefix' then lifetime is set to configured 'ip6LinkPrefixAdvPreferredLifetime'. Otherwise, it is set to minimum of configured value and inherited 'ip6PrefixAdvPreferredLifetime'.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH