>> MIB - Management Information Base
>> Table: biboAdmTrapHostTable - (.1.3.6.1.4.1.272.4.1.10.1)
Description: The biboAdmTrapHostTable defines where traps are sent (i.e., which hosts). If the table is empty traps are broadcasted. Creating entries: Entries are added by assigning an IP address value to the biboAdmTrapHostAddr field. Deleting entries: Entries can be removed by assigning ing the respective biboAdmTrapHostStatus field to 'delete'.
biboAdmTrapHostTable
OID | Name | Type | Access
.1 | Addr | IpAddress | RW
.2 | Status | ENUM | D
Addr
Ip-Address where traps are sent.
Status
Status is always valid, and set to delete only to discard the whole entry. Enumerations: valid (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH