>> MIB - Management Information Base
>> Table: ethoaPvcTable - (.1.3.6.1.4.1.272.4.16.15.1)
Description: The ethoaPvcTable displays all virtual ethernets defined for a VCI/VPI on a specified hardware.
ethoaPvcTable
OID | Name | Type | Access
.1 | IfIndex | Integer32 | R
.2 | Descr | DisplayString | RW
.3 | AtmIfIndex | Integer32 | RW
.4 | Vpi | INTEGER | RW
.5 | Vci | INTEGER | RW
.6 | Encapsulation | ENUM | D
.7 | PhysAddress | PhysAddress | RW
IfIndex
This object contains an interface index and assigns the row to an entry in ifTable. When creating new entries in the table, the value of this object shall be set to 0. The next free ifIndex value is than allocated and assigned to the object. At the same time a new interface is created in the IfTable.
Descr
Short description of the configured PVC Length: 0 to 255
AtmIfIndex
The Index to the ATM hardware.
Vpi
The VPI value of this Virtual Path Connection. Range: 0 to 255
Vci
The VCI value of this Virtual Channel Connection. Range: 0 to 65535
Encapsulation
This values decides whether frames are send without FCS(1), with FCS(2) or wether VC multiplexing is used. Enumerations: bridged-no-fcs (1) bridged-fcs (2) vc-multiplexed (3) delete (10)
PhysAddress
The MAC-Address used for the virtual interface.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH