>> MIB - Management Information Base
>> Table: x25CallHistoryTable - (.1.3.6.1.4.1.272.4.6.4.1)
Description: Entries are created automatically, when a call is cleared completely. The first entry is deleted automatcally, if a new entry would be the 11th entry in the table.
x25CallHistoryTable
OID | Name | Type | Access
.1 | Time | Date | R
.2 | Duration | INTEGER | R
.3 | SrcIfIndex | INTEGER | R
.4 | SrcLinkAddr | OCTET STRING | R
.5 | SrcVCNumber | INTEGER | R
.6 | DstIfIndex | INTEGER | R
.7 | DstLinkAddr | OCTET STRING | R
.8 | DstVCNumber | INTEGER | R
.9 | SrcAddr | DisplayString | R
.10 | DstAddr | DisplayString | R
.11 | ProtocolId | INTEGER | R
.12 | Facilities | OCTET STRING | R
.13 | UserData | DisplayString | R
.14 | InPktSize | ENUM | R
.15 | OutPktSize | ENUM | R
.16 | InWinSize | INTEGER | R
.17 | OutWinSize | INTEGER | R
.18 | PktsSent | Counter | R
.19 | BytesSent | Counter | R
.20 | PktsRecvd | Counter | R
.21 | BytesRecvd | Counter | R
.22 | ClearCause | INTEGER | R
.23 | ClearDiag | INTEGER | R
Time
Date and time, when the call was received. Range: 0 to -1
Duration
Duration of the call in seconds.
SrcIfIndex
Interface index of the link, the call came from.
SrcLinkAddr
(MAC-)address of the link, the call came from.
SrcVCNumber
Virtual Curcuit Number on the link, the call came from. Range: 1 to 4095
DstIfIndex
Interface index of the link, the call leads to.
DstLinkAddr
(MAC-)address of the link, the call leads to.
DstVCNumber
Virtual Curcuit Number on the link, the call leads to. Range: 1 to 4095
SrcAddr
The calling party number as received from the source link. Length: 0 to 255
DstAddr
The called party number as received from the source link. Length: 0 to 255
ProtocolId
The Protocol ID of the call (first four bytes of the call user data field) as received from the source link.
Facilities
The facility field of the call as received from the source link.
UserData
The call user data behind the protocol ID as received from the source link Length: 0 to 255
InPktSize
The packet size of packets being received by the caller, as negotiated by the negotiation procedure. Enumerations: p2 (1) p4 (2) p8 (3) p16 (4) p32 (5) p64 (6) p128 (7) p256 (8) p512 (9) p1024 (10) p2048 (11) p4096 (12) p8192 (13) p16384 (14) p32768 (15)
OutPktSize
The packet size of packets being sent by the caller, as negotiated by the negotiation procedure. Enumerations: p2 (1) p4 (2) p8 (3) p16 (4) p32 (5) p64 (6) p128 (7) p256 (8) p512 (9) p1024 (10) p2048 (11) p4096 (12) p8192 (13) p16384 (14) p32768 (15)
InWinSize
The window size of packets being received by the caller, as negotiated by the negotiation procedure. Range: 1 to 127
OutWinSize
The window size of packets being sent by the caller, as negotiated by the negotiation procedure. Range: 1 to 127
PktsSent
The number of all layer 3 packets (including RR/RNR/REJ) sent by the caller.
BytesSent
The number of data bytes sent in DATA and INTERRUPT packets by the caller.
PktsRecvd
The number of all layer 3 packets (including RR/RNR/REJ) received by the caller.
BytesRecvd
The number of data bytes received in DATA and INTERRUPT packets by the caller.
ClearCause
The clearing cause of the call as received in the first clear packet. A value of -1 means, no cause was received. Range: -1 to 255
ClearDiag
The clearing diagnostics of the call as received in the first clear packet. A value of -1 means, no diagnostics was received. Range: -1 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH