>> MIB - Management Information Base
>> Table: capi - (.1.3.6.1.4.1.272.4.7)
capi
OID | Name | Type | Access
.9 | AdminStatus | ENUM | RW
.10 | TcpNoDelay | ENUM | RW
.11 | FaxG3Header | ENUM | RW
.12 | X25DefWinSize | INTEGER | RW
AdminStatus
Enable or disable CAPI Enumerations: enable (1) disable (2)
TcpNoDelay
Enable or Disable TCP Nagle Algorithm for CAPI. disable: Normal operation with Nagle support. enable : Disable Nagle TCP Algorithm. Enable TcpNoDelay increases Network load and decrease delay of TCP packages. On CAPI Applications with small Data packages this option may increase transmission rate. Enumerations: enable (1) disable (2)
FaxG3Header
Specifies whether the header-line and logo ('BIANCA/FAX'), should appear on outgoing facsimiles. The value 'logo_header' allows the header-line and the logo to be printed on the top of each page. Enumerations: logo-header (1) no-logo (2) no-header (3) not-available (4) specify (5)
X25DefWinSize
Specifies the X.25 default Windowsize used in ISO8208 (X.25 DTE <-> DTE) Filetransferprotocol. Applications such as OFTP normally uses 7 but some Applications did not use X.25 negotiation, so the CAPI uses here a default from 2 and the connection is closed by a X.25 Reset. Setting this value to 7 is not standard but useful for the customer to avoid this error. Range: 1 to 7

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH