>> MIB - Management Information Base
>> Table: wlcClientProfileTable - (.1.3.6.1.4.1.272.4.61.1.18.1)
Description: This table contains WTP radio client profiles.
wlcClientProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | ScanPeriodAMin | INTEGER | RW
.3 | ScanPeriodAMax | INTEGER | RW
.4 | ScanPeriodMin | INTEGER | RW
.5 | ScanPeriodMax | INTEGER | RW
.7 | AdminStatus | ENUM | D
Index
Unique Client profile index.
ScanPeriodAMin
Minimum time in ms to spend on a frequency when active scanning. Default is 10ms.
ScanPeriodAMax
Maximum time in ms to spend on a frequency when active scanning. Default is 40ms.
ScanPeriodMin
Minimum time in ms to spend on a frequency when passive scanning. Default is 20ms.
ScanPeriodMax
Maximum time in ms to spend on a frequency when passive scanning. Default is 120ms.
AdminStatus
Enable or delte the requested WLAN client profile. Enumerations: enabled (1) delete (32)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH