>> MIB - Management Information Base
>> Table: ipNetToMediaTable - (.1.3.6.1.2.1.4.22.1)
Description: Each entry contains one IpAddress to `physical' address equivalence.
ipNetToMediaTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RC
.2 | PhysAddress | PhysAddress | RC
.3 | NetAddress | IpAddress | RC
.4 | Type | ENUM | D
IfIndex
The interface on which this entry's equivalence is effective. The interface identified by a particular value of this index is the same interface as identified by the same value of the IF-MIB's ifIndex. This object predates the rule limiting index objects to a max access value of 'not-accessible' and so continues to use a value of 'read-create'. Range: 1 to 2147483647
PhysAddress
The media-dependent `physical' address. This object should return 0 when this entry is in the 'incomplete' state. As the entries in this table are typically not persistent when this object is written the entity should not save the change to non-volatile storage. Note: a stronger requirement is not used because this object was previously defined. Length: 0 to 65535
NetAddress
The IpAddress corresponding to the media-dependent `physical' address. This object predates the rule limiting index objects to a max access value of 'not-accessible' and so continues to use a value of 'read-create'.
Type
The type of mapping. Setting this object to the value invalid(2) has the effect of invalidating the corresponding entry in the ipNetToMediaTable. That is, it effectively dis-associates the interface identified with said entry from the mapping identified with said entry. It is an implementation- specific matter as to whether the agent removes an invalidated entry from the table. Accordingly, management stations must be prepared to receive tabular information from agents that corresponds to entries not currently in use. Proper interpretation of such entries requires examination of the relevant ipNetToMediaType object. As the entries in this table are typically not persistent when this object is written the entity should not save the change to non-volatile storage. Note: a stronger requirement is not used because this object was previously defined. Enumerations: other (1) invalid (2) dynamic (3) static (4)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH