>> MIB - Management Information Base
>> Table: biboAdmBoardTable - (.1.3.6.1.4.1.272.4.1.17.1)
Description: The biboAdmBoardTable lists information about the installed communications modules. This table is updated after every system boot up. Creating entries: Entries are created by the system upon detecting the installed hardware. Deleting entries: Entries are removed by the system as a result of removed hardware.
biboAdmBoardTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Type | DisplayString | R
.3 | HWRelease | DisplayString | R
.4 | FWRelease | DisplayString | R
.5 | PartNo | DisplayString | R
.6 | Connector | ENUM | RW
.7 | Unit | INTEGER | R
.8 | SerialNo | DisplayString | R
.9 | Category | ENUM | R
Slot
The slot, or location of this module. Range: 0 to 31
Type
The name of this module. Length: 0 to 255
HWRelease
The hardware release of this module. Length: 0 to 255
FWRelease
The firmware release of this module. Length: 0 to 255
PartNo
The part number of this module. Length: 0 to 255
Connector
The type of connector used for this module. For modules with more than one connector this value can be changed/switched by setting this object. For example, the CM-BNCTP module supports both twisted pair (RJ45) and 10Base2 (BNC) connectors. If this object is set to 'AUTO' then the BRICK will automatically detect which connector type is being used. Enumerations: auto (1) rj45 (2) bnc (3) subd15 (4) rj45-10mbit-hdup (5) rj45-10mbit-fdup (6) rj45-100mbit-hdup (7) rj45-100mbit-fdup (8)
Unit
The logical unit number of this interface. Range: 0 to 99
SerialNo
The serial number of this module. Length: 0 to 255
Category
Board category. It can be one of the following: system-board(1), ethernet(2), isdn-bri(3), isdn-pmx(4), pots(5), dsl(6), wlan(7), tty(8), dsp(9), usb(10), crypt(11), mobile(12) It advices users of which MIB table to look at when searching for additional configuration informations. Enumerations: system-board (1) ethernet (2) isdn-bri (3) isdn-pmx (4) pots (5) dsl (6) wlan (7) tty (8) dsp (9) usb (10) crypt (11) mobile (12)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH