>> MIB - Management Information Base
>> Table: ip6DsLiteTable - (.1.3.6.1.4.1.272.4.5.100.1.9.1)
Description: Contains a DsLite (4in6) configuration.
ip6DsLiteTable
OID | Name | Type | Access
.1 | IfIndexV4 | InterfaceIndexOrZero | RW
.2 | IfIndexV6 | InterfaceIndex | RW
.3 | Descr | DisplayString | RW
.4 | ConfigMode | ENUM | D
.5 | Encapsulation | ENUM | RW
.6 | LocalAddress | InetAddressIPv6 | RW
.7 | RemoteAddress | InetAddressIPv6 | RW
.8 | UsedLocalAddress | InetAddressIPv6 | R
.9 | UsedRemoteAddress | InetAddressIPv6 | R
.10 | AftrFqdn | DisplayString | RW
.11 | AftrDynFqdn | DisplayString | R
.12 | NextRetry | INTEGER | R
IfIndexV4
Unique Identifier for this entry Range: 0 to 2147483647
IfIndexV6
Specifies the associated IPv6 interface for this entry. Range: 1 to 2147483647
Descr
Description for the DsLite connection Length: 0 to 255
ConfigMode
Configuration mode of the tunnel addresse. Enumerations: static (1) dhcp (2) delete (8)
Encapsulation
The encapsulation used for this tunnel. Enumerations: ipip (1) none (16)
LocalAddress
Static configured local IPv6 address of ithis tunnel. Length: 16 to 16
RemoteAddress
DsLite tunnel endpoint IPv6 address. Length: 16 to 16
UsedLocalAddress
Used local IPv6 address of this tunnel. Length: 16 to 16
UsedRemoteAddress
Used tunnel endpoint IPv6 address of this tunnel. Length: 16 to 16
AftrFqdn
FQDN of the associated Address Family Transition Router (AFTR). Will be used and resolved as long as there is no static AFTR address (ip6DsLiteRemoteAddress) given. Length: 0 to 255
AftrDynFqdn
FQDN of the associated Address Family Transition Router (AFTR). If ip6DsLiteConfigMode is set to dhcp(2) this name will be requested via DHCPv6 (option 64 according RFC 6334), and if provided by the DHCP server it will be used as long as there is no static AFTR address (ip6DsLiteRemoteAddress) given. Length: 0 to 255
NextRetry
Time in seconds til next try to resolve the AFTR FQDN. Range: 0 to 60

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH