>> MIB - Management Information Base
>> Table: mobileOperatorPLMNTable - (.1.3.6.1.4.1.272.4.41.4.1.28.1)
Description: A single mobileOperatorPLMNTable entry.
mobileOperatorPLMNTable
OID | Name | Type | Access
.1 | IccId | DisplayString | R
.2 | Code | INTEGER | R
.3 | Name | DisplayString | R
.4 | AllowGSM | ENUM | R
.5 | AllowUMTS | ENUM | R
IccId
The ICC-ID of the SIM-Card. The Operator PLMN List is copied from this SIM-Card. Length: 0 to 20
Code
The PLMN Code is built from a 3 digit MCC (Mobile Country Code) and 2 or 3 digit MNC (Mobile Network Code).
Name
The name of the network operator. Length: 0 to 40
AllowGSM
The Access Right to register to GSM Access Technology. Enumerations: allowed (1) denied (2)
AllowUMTS
The Access Right to register to UMTS Access Technology. Enumerations: allowed (1) denied (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH