>> MIB - Management Information Base
>> Table: ip6DhcpStatefulClientTable - (.1.3.6.1.4.1.272.4.5.100.4.11.1)
Description: DHCPv6-clients with currently assigned address, prefix, or FQDN.
ip6DhcpStatefulClientTable
OID | Name | Type | Access
.1 | DUID | OCTET STRING | R
.2 | Name | DisplayString | R
.3 | Age | TimeStamp | R
.4 | LastUpdate | TimeStamp | R
DUID
DUID of DHCPv6-client (see 9 and 22.2 of RFC-3315). An empty dummy-DUID is used for storing addresses from received Decline-messages (see section 5.3 of RFC-33).
Name
Partial or fully qualified domain-name, if provided by client, otherwise empty. Value is overridden by 'Name' of related 'ip6DhcpClientFqdnOpt' entry, if existing and not empty. Length: 0 to 255
Age
Age of this client-entry.
LastUpdate
Timestamp for latest update of this client-entry.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH