>> MIB - Management Information Base
>> Table: mpsSwitchingContactTable - (.1.3.6.1.4.1.272.4.53.18.1.1)
Description: Settings for each switching contact
mpsSwitchingContactTable
OID | Name | Type | Access
.1 | Index | SwitchingContactIndex | R
.2 | Description | DisplayString | RW
.3 | Type | ENUM | RW
.4 | Timer | INTEGER | RW
Index
A unique value for each switching contact (relay number). Range: 1 to 2
Description
A description for this switching contact Length: 0 to 255
Type
This value defines the application for which the switching contact is used: dial-code(1) : Contact is controlled according to used dial codes (on/off or closed for a period of time). alarm-output(2) : Contact is actuated during an alarm call. voice-announcement(3) : Contact is actuated during an ongoing voice announcement. dial-code-period-only(4): Contact only actuated by dial code for closing a period of time. dial-code-toggle-only(5): Contact only actuated by dial codes for switching on/off. Enumerations: dial-code (1) alarm-output (2) voice-announcement (3) dial-code-period-only (4) dial-code-toggle-only (5)
Timer
Switching contact signalling period in seconds. Range: 1 to 999

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH