>> MIB - Management Information Base
>> Table: wlanVSSExtTable - (.1.3.6.1.4.1.272.4.46.38.1)
Description: The wlanVSSExtTable contains extended information related to the VSS configured in the device. Entries can only be added or deleted by the system.
wlanVSSExtTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | RSSIThresholdValue | INTEGER | RW
.3 | RSSIThresholdGraceTime | INTEGER | RW
IfIndex
Unique VSS index.
RSSIThresholdValue
Defines the signal threshold used to disassociate all the stations with lesser signal than the defined value.
RSSIThresholdGraceTime
The stations with RSSI lower than the threshold will be dropped after exhausting this amount of time. If 0, the stations will be dropped immediately

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH