>> MIB - Management Information Base
>> Table: pptpCallTable - (.1.3.6.1.4.1.272.4.23.3.1)
Description: The pptpCallTable displays all currently active PPTP calls (incoming and outgoing). Only the system can add or remove entries to this table. Creating entries: Entries are added when an outgoing call is made or when an incoming call is connected. Deleting entries: Entries are removed once the respective call is disconnected.
pptpCallTable
OID | Name | Type | Access
.1 | Type | ENUM | R
.2 | Direction | ENUM | R
.3 | Age | TimeTicks | R
.4 | State | ENUM | D
.5 | RemoteIpAddress | IpAddress | R
.6 | LocalIpAddress | IpAddress | R
.7 | ReceivedPackets | Counter | R
.8 | ReceivedOctets | Counter | R
.9 | ReceivedErrors | Counter | R
.10 | TransmitPackets | Counter | R
.11 | TransmitOctets | Counter | R
.12 | TransmitErrors | Counter | R
.13 | Info | DisplayString | R
.14 | LocId | INTEGER | R
.15 | RemId | INTEGER | R
.16 | Serial | INTEGER | R
.17 | SWin | INTEGER | R
.18 | GreWindowAdaption | ENUM | R
.19 | AssociatedIfIndex | INTEGER | R
Type
The PPTP call type. Enumerations: pac (1) pns (2)
Direction
Direction of the PPTP call, incoming(1) or outgoing(2). Enumerations: incoming (1) outgoing (2)
Age
The age of the call. For outgoing calls, the time since the call began, or for incoming calls, the time since the call was received. The format is in hh:mm:ss.00.
State
The state of the PPTP call according RFC 2637. Enumerations: idle (1) wait-cs-ans (2) wait-reply (3) wait-connect (4) established (5) wait-disc (6) close (7) delete (8)
RemoteIpAddress
The called (for outgoing calls) or calling IP address (for incoming calls).
LocalIpAddress
The calling (for outgoing calls) or called IP address (for incoming calls).
ReceivedPackets
Count of received valid GRE-encapsulated packets.
ReceivedOctets
Count of received valid Octets.
ReceivedErrors
Count of received invalid GRE-encapsulated packets.
TransmitPackets
Count of transmitted GRE-encapsulated packets.
TransmitOctets
Count of transmitted Octets.
TransmitErrors
Count of transmit errors.
Info
Additional information to identify the PPTP call. Length: 0 to 255
LocId
The local PPTP call ID assigned by remote.
RemId
The locally assigned remote PPTP call ID.
Serial
The unique Call Serial Number. Unlike the Call ID, both the PNS and PAC associate the same Call Serial Number with a given session
SWin
The negotiated GRE send window size Range: 0 to 256
GreWindowAdaption
Displays wether the sliding GRE window algorithm is enabled or disabled. Enumerations: enabled (1) disabled (2)
AssociatedIfIndex
The index of the associated virtual interface.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH