>> MIB - Management Information Base
>> Table: ipsecRadius - (.1.3.6.1.4.1.272.4.26.13)
ipsecRadius
OID | Name | Type | Access
.1 | PresetState | ENUM | R
.2 | PresetPeers | INTEGER | R
.3 | DynamicAuthentication | ENUM | RW
PresetState
This object shows the status of the RADIUS preset peers load process.
PresetPeers
The number of RADIUS preset peers currently loaded.
DynamicAuthentication
This object enables/disables dynamic authentication via RADIUS. If no peer has been found matching an incoming IKE negotiation, the configured RADIUS servers are consulted (if any).

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH