>> MIB - Management Information Base
>> Table: pppoaPvcTable - (.1.3.6.1.4.1.272.4.16.17.1)
Description: This table configures Vpi/Vci for PPP oaver AAL5 (PPPoA) permanent and on-demand sessions.
pppoaPvcTable
OID | Name | Type | Access
.1 | IfIndex | Integer32 | R
.2 | Descr | DisplayString | RW
.3 | AtmIfIndex | Integer32 | RW
.4 | Vpi | INTEGER | RW
.5 | Vci | INTEGER | RW
.6 | Encapsulation | ENUM | D
.7 | ClientType | ENUM | RW
IfIndex
This object contains an interface index and refers to an entry in ifTable. When creating new entries in the table, the next free ifIndex value is than allocated and assigned to the object. At the same time a new interface is created in the IfTable with that very index.
Descr
Short description of the configured PVC Length: 0 to 255
AtmIfIndex
The Index to the ATM hardware.
Vpi
The VPI value of this Virtual Path Connection. Range: 0 to 255
Vci
The VCI value of this Virtual Channel Connection. Range: 0 to 65535
Encapsulation
This value decides whether VC multiplexing or LLC encapsulation is used. Enumerations: vc-multiplexed (1) llc (2) delete (10)
ClientType
This variable defines whether the PPP over AAL5 session will be established permanent(1) or initiated on-demand(2). Enumerations: permanent (1) on-demand (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH