>> MIB - Management Information Base
>> Table: mpsSystemNumberTable - (.1.3.6.1.4.1.272.4.53.2.6.1)
Description: This table contains additional system numbers.
mpsSystemNumberTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Type | ENUM | RW
.3 | Number | DisplayString | RW
.4 | AdminStatus | ENUM | D
.5 | Position | Unsigned32 | RW
Index
A unique value for each system number.
Type
Type of system number. service-number(1) : internal service number. trunk-access(2) : line access digit to external line. pickup(3) : pickup an internal call. specific-pickup(4) : pickup an internal call via extension number. project-code(5) : stored in accounting data. speed-dial(6) : telephone call via speed dial number. open-inquiry(7) : system parking number. bundle-req(8) : access code for external trunk bundles. systel-update-fw(9) : update system phone firmware. Enumerations: service-number (1) trunk-access (2) pickup (3) specific-pickup (4) project-code (5) speed-dial (6) open-inquiry (7) bundle-req (8) systel-update-fw (9)
Number
The digits of the system number. Length: 0 to 16
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
Position
A counter for open-inquiry(7) and bundle-req(8) (mpsSystemNumberType). If mpsSystemNumberType = bundle-req, mpsSystemNumberPosition referecenes to mpsTrunkBundleTable.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH