>> MIB - Management Information Base
>> Table: sshdSessionTable - (.1.3.6.1.4.1.272.4.44.2.1)
Description: A list of the currently active clients of sshd.
sshdSessionTable
OID | Name | Type | Access
.1 | TimeStamp | Date | R
.2 | State | ENUM | D
.3 | IpAddr | IpAddress | R
.4 | IpPort | INTEGER | R
.5 | Cipher | DisplayString | R
.6 | Mac | DisplayString | R
.7 | BytesIn | INTEGER | R
.8 | BytesOut | INTEGER | R
.9 | UserName | DisplayString | R
.10 | Compression | DisplayString | R
.11 | RemAddrType | ENUM | R
.12 | RemAddr | InetAddress | R
TimeStamp
The timestamp for the TCP connection establishment. Range: 0 to -1
State
The connection state of this client. Enumerations: new (1) authenticating (2) connected (3) disconnecting (4) delete (15)
IpAddr
The IP address of this client. Only used for IPv4.
IpPort
The associated port # of this client.
Cipher
The cipher negotiated with this client. Length: 0 to 255
Mac
The MAC (message authentication code) negotiated with this client. Length: 0 to 255
BytesIn
The # of bytes received from this client.
BytesOut
The # of bytes send to this client.
UserName
The account used for the client's successful login. Length: 0 to 255
Compression
The compression algorithm negotiated with this client. Length: 0 to 255
RemAddrType
The address-type of this client (remote address). Related address is given in sshdSessionRemAddr. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
RemAddr
The Internet-address of this client (remote address). Related address-type is given in sshdSessionRemAddrType. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH