>> MIB - Management Information Base
>> Table: ospfGeneralGroup - (.1.3.6.1.2.1.14.1)
ospfGeneralGroup
OID | Name | Type | Access
.1 | RouterId | IpAddress | R
.2 | AdminStat | ENUM | RW
.3 | VersionNumber | ENUM | R
.4 | AreaBdrRtrStatus | ENUM | R
.5 | AsBdrRtrStatus | ENUM | R
.6 | ExternLsaCount | Gauge | R
.7 | ExternLsaCksumSum | HexValue | R
.8 | TOSSupport | ENUM | R
.9 | OriginateNewLsas | Counter | R
.10 | RxNewLsas | Counter | R
.11 | ExtLsdbLimit | INTEGER | RW
.12 | MulticastExtensions | INTEGER | R
.13 | ExitOverflowInterval | INTEGER | RW
.14 | DemandExtensions | ENUM | R
RouterId
A 32-bit integer uniquely identifying the router in the Autonomous System. By convention, to ensure uniqueness, this should default to the value of one of the router's IP interface addresses.
AdminStat
The administrative status of OSPF in the router. The value 'enabled' denotes that the OSPF Process is active on at least one interface; 'disabled' disables it on all interfaces. Enumerations: enabled (1) disabled (2)
VersionNumber
The current version number of the OSPF protocol is 2. Enumerations: undef (1) version2 (2)
AreaBdrRtrStatus
A flag to note whether this router is an area border router. Enumerations: true (1) false (2)
AsBdrRtrStatus
A flag to note whether this router is an Autonomous System border router. Enumerations: true (1) false (2)
ExternLsaCount
The number of external (LS type 5) link-state advertisements in the link-state database.
ExternLsaCksumSum
The 32-bit unsigned sum of the LS checksums of the external link-state advertisements contained in the link-state database. This sum can be used to determine if there has been a change in a router's link state database, and to compare the link-state database of two routers. Range: 0 to -1
TOSSupport
The router's support for type-of-service routing. Enumerations: true (1) false (2)
OriginateNewLsas
The number of new link-state advertisements that have been originated. This number is incremented each time the router originates a new LSA.
RxNewLsas
The number of link-state advertisements received determined to be new instantiations. This number does not include newer instantiations of self-originated link-state advertisements.
ExtLsdbLimit
The maximum number of non-default AS- external-LSAs entries that can be stored in the link-state database. If the value is -1, then there is no limit. When the number of non-default AS-external-LSAs in a router's link-state database reaches ospfExtLsdbLimit, the router enters Overflow- State. The router never holds more than ospfExtLsdbLimit non-default AS-external-LSAs in its database. OspfExtLsdbLimit MUST be set identically in all routers attached to the OSPF backbone and/or any regular OSPF area. (i.e., OSPF stub areas and NSSAs are excluded).
MulticastExtensions
A Bit Mask indicating whether the router is forwarding IP multicast (Class D) datagrams based on the algorithms defined in the Multi- cast Extensions to OSPF. Bit 0, if set, indicates that the router can forward IP multicast datagrams in the router's directly attached areas (called intra-area mul- ticast routing). Bit 1, if set, indicates that the router can forward IP multicast datagrams between OSPF areas (called inter-area multicast routing). Bit 2, if set, indicates that the router can forward IP multicast datagrams between Auto- nomous Systems (called inter-AS multicast rout- ing). Only certain combinations of bit settings are allowed, namely: 0 (no multicast forwarding is enabled), 1 (intra-area multicasting only), 3 (intra-area and inter-area multicasting), 5 (intra-area and inter-AS multicasting) and 7 (multicasting everywhere). By default, no mul- ticast forwarding is enabled.
ExitOverflowInterval
The number of seconds that, after entering OverflowState, a router will attempt to leave OverflowState. This allows the router to again originate non-default AS-external-LSAs. When set to 0, the router will not leave Overflow- State until restarted.
DemandExtensions
The router's support for demand routing. Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH