>> MIB - Management Information Base
>> Table: isdnCallTable - (.1.3.6.1.4.1.272.4.2.4.1)
Description: The isdnCallTable displays all currently active ISDN calls (incoming and outgoing). Only the system can add or remove entries to this table. Creating entries: Entries are added when an outgoing call is made or when an incoming call is connected. Deleting entries: Entries are removed once the respective call is disconnected.
isdnCallTable
OID | Name | Type | Access
.1 | StkNumber | INTEGER | R
.2 | Type | ENUM | R
.3 | Reference | INTEGER | R
.4 | Age | TimeTicks | R
.5 | State | ENUM | RW
.6 | IsdnIfIndex | INTEGER | R
.7 | Channel | INTEGER | R
.8 | DspItem | ENUM | R
.9 | RemoteNumber | DisplayString | R
.10 | RemoteSubaddress | OCTET STRING | R
.11 | LocalNumber | DisplayString | R
.12 | LocalSubaddress | OCTET STRING | R
.13 | ServiceIndicator | ENUM | R
.14 | AddInfo | INTEGER | R
.15 | BC | OCTET STRING | R
.16 | LLC | OCTET STRING | R
.17 | HLC | OCTET STRING | R
.18 | Charge | INTEGER | R
.19 | ReceivedPackets | Counter32 | R
.20 | ReceivedOctets | Counter32 | R
.21 | ReceivedErrors | Counter32 | R
.22 | TransmitPackets | Counter32 | R
.23 | TransmitOctets | Counter32 | R
.24 | TransmitErrors | Counter32 | R
.25 | ChargeInfo | DisplayString | R
.26 | Screening | ENUM | R
.27 | Info | DisplayString | R
.28 | ReceiveDiscards | Counter32 | R
.29 | AssociatedIfIndex | INTEGER | R
StkNumber
The number of the ISDN-Stack, this call is going through. Refer to the isdnStkTable. Range: 0 to 31
Type
The direction of the call. Enumerations: incoming (1) outgoing (2)
Reference
The corresponding Call-Reference Value on the ISDN D-channel.
Age
The age of the call. For outgoing calls, the time since the call began, or for incoming calls, the time since the call was received. The format is in hh:mm:ss.00.
State
The state of the call. Enumerations: null (1) c-initiated (2) ovl-send (3) oc-procd (4) c-deliverd (5) c-present (7) c-recvd (8) con-req (9) ic-procd (10) active (11) discon-req (12) discon-ind (13) suspd-req (16) resum-req (18) rel-req (20) ovl-recv (26)
IsdnIfIndex
The corresponding ISDN interface that is used for this call. Refer to the isdnIfTable.
Channel
The corresponding B-channel on this ISDN interface. Refer to the isdnIfTable. Range: 0 to 31
DspItem
The item to or from which this call is connected. For any routing tasks (IP, IPX, X.25, bridging, ...) the ppp(1) item is used. For the isdnlogin program, login(2) is used. For CAPI 1.1 programs, the items eaz0(48) .. eaz9(57) are used. Enumerations: ppp (1) login (2) undefined (10) ppp-64k (11) ppp-56k (12) ppp-modem (13) ppp-dovb (14) ppp-v110-1200 (15) ppp-v110-2400 (16) ppp-v110-4800 (17) ppp-v110-9600 (18) ppp-v110-14400 (19) ppp-v110-19200 (20) ppp-v110-38400 (21) ppp-x75 (22) ppp-v120 (23) pots (25) ppp-modem-profile-1 (26) ppp-modem-profile-2 (27) ppp-modem-profile-3 (28) ppp-modem-profile-4 (29) ppp-modem-profile-5 (30) ppp-modem-profile-6 (31) ppp-modem-profile-7 (32) ppp-modem-profile-8 (33) ppp-dovb-64k (34) eaz0 (48) eaz1 (49) eaz2 (50) eaz3 (51) eaz4 (52) eaz5 (53) eaz6 (54) eaz7 (55) eaz8 (56) eaz9 (57) x25-pad (58) capi2 (59) ipsec (60) x25 (61) service-call (62)
RemoteNumber
The ISDN number that was called (for outgoing calls) or was calling (for incoming calls). Length: 0 to 255
RemoteSubaddress
The subaddress of the remote number. The subaddress is coded in NSAP format as octets. See isdnCallRemoteNumber.
LocalNumber
The calling party number that was sent (with the outgoing call) or was received (with incoming calls). Refer to the isdnStkTable. Length: 0 to 255
LocalSubaddress
The subaddress of the calling party number. See isdnCallRLocalNumber.
ServiceIndicator
Service indicator that was sent on the ISDN D-channel when the call was established. Enumerations: telephony (1) ab-services (2) x21-services (3) fax-group4 (4) btx (5) data-transfer (7) x25-services (8) facsimile64 (9) mixed-mode (10) telecontrol (13) graphics-phone (14) teletex (15) video-phone (16)
AddInfo
Additional information that was sent on the ISDN D-channel when the call was established. Only sent/received when using the 1TR6 protocol. Range: 0 to 255
BC
Bearer Capability that was sent on the ISDN D-channel when the call was established.
LLC
Low Layer Capability that was sent on the ISDN D-channel when the call was established.
HLC
The number of charging ticks received since this connection was established. Actual charges can be computed by multiplying this value with the unit price (e.g. .12 DM in Germany). If you aren't receiving charging information for outgoing calls, verify with your local ISDN provider to make sure this option is being provided/is available.
Charge
This object contains the charge for this call either as units or as 1/1000 of the respective currency. Which type of information is choosen, depends on the information provided by the ISDN service provide. See also ChargeInfo for textual information.
ReceivedPackets
Count of received valid HDLC Frames.
ReceivedOctets
Count of received valid HDLC Octets.
ReceivedErrors
Count of received invalid HDLC Frames.
TransmitPackets
Count of transmitted HDLC Frames.
TransmitOctets
Count of transmitted Octets.
TransmitErrors
Count of transmit errors (Collision, TX underrun).
ChargeInfo
Textual information of charge, i.e. 0.12 DM or 3 units Length: 0 to 255
Screening
Screening Indicator of the calling party number of incoming calls. The calling partys number (CPN) may be assigned either by the user placing the call or by the telephone switching station. If the CPN was assigned by the user the switching station may optionally verify the address. indicator: CPN assigned: verification: `user' by user none `user-verified' by user verification successful `user-failed' by user verification failed `network' by network none Enumerations: user (1) user-verified (2) user-failed (3) network (4) undefined (5)
Info
Additional information to identify the call Length: 0 to 255
ReceiveDiscards
Count of received and discarded data frames.
AssociatedIfIndex
The index of the associated virtual interface.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH