>> MIB - Management Information Base
>> Table: voipEmergencyTable - (.1.3.6.1.4.1.272.4.33.21.1)
Description: Describes an emergency rule
voipEmergencyTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | AdminStatus | ENUM | D
.3 | Descr | DisplayString | RW
.4 | Number | DisplayString | RW
.5 | Interface | INTEGER | RW
.6 | Convert | DisplayString | RW
Index
The unique Index value for this entry. Range: 1 to 65535
AdminStatus
The administrative state of this entry. Enumerations: enabled (1) disabled (2) delete (3)
Descr
Description of this entry. Length: 0 to 255
Number
The emergency Number for handling Length: 0 to 255
Interface
Optional: The fixed outgoing VoIP Interface for this emergency address, independent from any other call routing. Default: If this value is 0, the standard call routing is used to retrieve the outgoing interface but any conversion rules specified in the call routing entry are skipped and only the numbers defined in this entry are dialed instead.
Convert
Optional: The new emergency number if the outgoing interface uses a different emergency format. Default: Empty. No conversion is done. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH