>> MIB - Management Information Base
>> Table: ipSifRejectTable - (.1.3.6.1.4.1.272.4.5.31.1)
Description: Contains actually rejected Frames with Source Destination
ipSifRejectTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Source | IpAddress | R
.3 | Destination | IpAddress | R
.4 | Rejects | INTEGER | R
.5 | Silence | INTEGER | R
.6 | Protocol | INTEGER | R
.7 | PortLo | INTEGER | R
.8 | PortHigh | INTEGER | R
.10 | SrcType | ENUM | R
.11 | Src | InetAddress | R
.12 | DstType | ENUM | R
.13 | Dst | InetAddress | R
Index
Unique index for this entry.
Source
The Reject Source for the Entry
Destination
The Reject Destination Index for the Entry
Rejects
Number of rejected frames.
Silence
Last reject in seconds
Protocol
The IP protocol of the packet.
PortLo
The lowest UDP/TCP port number seen.
PortHigh
The highest UDP/TCP port number seen.
SrcType
The type of the source IP address. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Src
The source IP address. Length: 0 to 255
DstType
The type of the destination IP address. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Dst
The destination IP address. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH