>> MIB - Management Information Base
>> Table: serviceCallAdmin - (.1.3.6.1.4.1.272.4.22.8.1)
serviceCallAdmin
OID | Name | Type | Access
.1 | DaemonAdminStatus | ENUM | RW
.2 | DaemonOperStatus | ENUM | R
.3 | ServiceHostAddress | DisplayString | RW
.4 | ServiceHostPort | INTEGER | RW
.6 | DefaultShorthold | INTEGER | RW
.7 | KnownHostsFileName | DisplayString | RW
DaemonAdminStatus
Activate/deactivate service-call-daemon. Enumerations: enabled (1) disabled (2)
DaemonOperStatus
Current operational state of service-call-daemon. Enumerations: enabled (1) disabled (2)
ServiceHostAddress
Address or domain-name of to-be-called server for service-requests. Length: 0 to 255
ServiceHostPort
Control-channel port-number of to-be-called server.
DefaultShorthold
Time in seconds to wait before closing an inactive service-call.
KnownHostsFileName
Optional 'known_host' file-name to be set when starting SSH-client. If string not empty, SSH-client-variables 'GlobalKnownHostsFile' and 'UserKnownHostsFile' are set to it in order to override defaults. More details are listed in table 'sshcKnownHost'. WARNING: Due to parameter-parsing, string must not hold any blanks. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH