>> MIB - Management Information Base
>> Table: usbConfigDescTable - (.1.3.6.1.4.1.272.4.55.2.1)
Description: (one entry of usbConfigDescTable)
usbConfigDescTable
OID | Name | Type | Access
.1 | DevAddr | INTEGER | R
.2 | TotalLength | INTEGER | R
.3 | NumInterfaces | INTEGER | R
.4 | ConfigValue | INTEGER | R
.5 | TxtConfiguration | DisplayString | R
.6 | Attributes | INTEGER | R
.7 | MaxPower | INTEGER | R
.8 | RawData | OCTET STRING | R
DevAddr
DevAddr = (slot << 12) | (unit << 8) | (Enum << 4). Enum is assigned by the USB device enumerator. Range: 0 to 65535
TotalLength
Length of the configuration descriptor frame in bytes. Range: 0 to 65535
NumInterfaces
The number of interfaces supported by the USB device. Range: 0 to 255
ConfigValue
The configuration value associated with this configuration. Range: 0 to 255
TxtConfiguration
Human readable configuration description (if present). Length: 0 to 255
Attributes
The following attributes are currently defined by the USB standard: Bit 7 - bus powered Bit 6 - self powered Bit 5 - remote wakeup Bit 4-0 - reserved. Range: 0 to 255
MaxPower
Maximum power consumption in steps of 2 mA. Range: 0 to 255
RawData
Configuration descriptor raw data for debugging purposes only. Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH