>> MIB - Management Information Base
>> Table: mpsEmergencyNumberTable - (.1.3.6.1.4.1.272.4.53.2.1.1)
Description: This Table contains the numbers of emergency calls. Emergency numbers can be dialed, even if all B-channels of the PBX are busy.
mpsEmergencyNumberTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Target | DisplayString | RW
.3 | Descr | DisplayString | RW
.4 | AdminStatus | ENUM | D
Index
A unique value for each emergency number.
Target
Contains the emergency number. Length: 0 to 24
Descr
Contains the description of emergency number. Length: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH