>> MIB - Management Information Base
>> Table: mpsDoorIntercomModeChainTable - (.1.3.6.1.4.1.272.4.53.7.5.1)
Description: This table contains the extension of each door intercom group and variant.
mpsDoorIntercomModeChainTable
OID | Name | Type | Access
.1 | Index | DoorIntercomIndex | RW
.2 | Button | DoorButtonIndex | RW
.3 | Number | DoorIntercomModeIndex | RW
.4 | Position | Unsigned32 | RW
.5 | Extension | ExtensionIndex | RW
.6 | AdminStatus | ENUM | D
Index
A unique value for each door intercom. Reference to mpsDoorIntercomIndex. Range: 1 to 10
Button
A unique value for each door intercom. Reference to mpsDoorIntercomSourceButtonIndex. Range: 1 to 4
Number
For each door intercom a variant. Reference to mpsDoorIntercomUserMode. Range: 1 to 10
Position
This value determine the order of the called extensions.
Extension
A unique value for each extension in the door intercom group variant. Reference to mpsExtensionIndex in mpsExtensionTable. Range: 1 to 65535
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH