>> MIB - Management Information Base
>> Table: citPvcTable - (.1.3.6.1.4.1.272.4.16.23.1)
Description: This table configures Vpi/Vci for tunneling to CIT host.
citPvcTable
OID | Name | Type | Access
.1 | FlowId | INTEGER | RW
.2 | AtmIfIndex | Integer32 | RW
.3 | Vpi | INTEGER | RW
.4 | Vci | INTEGER | RW
.5 | AAL | ENUM | D
FlowId
FlowID used for multiplexing to CIT host.
AtmIfIndex
The Index to the ATM hardware.
Vpi
The VPI value of this Virtual Connection.
Vci
The VCI value of this Virtual Connection.
AAL
This value selects the AAL mode of the VC.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH