>> MIB - Management Information Base
>> Table: ipDropinIfTable - (.1.3.6.1.4.1.272.4.5.65.1)
Description: .
ipDropinIfTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Descr | DisplayString | RW
.3 | Group | INTEGER | RW
.4 | AdminStatus | ENUM | D
.5 | ExcludeFromNat | ENUM | RW
Index
Index of interface to be associated with drop-in group.
Descr
A textual string describing this IP drop-in interface. Length: 0 to 255
Group
Associated drop-in group.
AdminStatus
Administrative status in order to switch on/off the drop-in mode for the interface. Enumerations: enabled (1) disabled (2) delete (3)
ExcludeFromNat
This variable determines, in conjunction with the variable 'ipDropinGroupExcludeFromNat', whether the NAT procedure is bypassed for IP addresses (source or target) within the drop-in network - with exception of the address 'ipDropinGroupUsedLocalAddr' itself. If set to enabled (2) NAT-less communication initiated from or addressed to the drop-in network is possible, needed for non-private DMZ networks for example. Enumerations: disabled (1) enabled (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH