>> MIB - Management Information Base
>> Table: mpsCallerNumberTable - (.1.3.6.1.4.1.272.4.53.2.7.1)
Description: Blacklist for incoming calls / Call distribution by caller number.
mpsCallerNumberTable
OID | Name | Type | Access
.1 | Index | Unsigned32 | RW
.2 | Filter | DisplayString | RW
.3 | FilterDescr | DisplayString | RW
.4 | FilterType | ENUM | RW
.5 | Target | ENUM | RW
.6 | TargetIndex | INTEGER | RW
.7 | AnnFileDir | DisplayString | RW
.8 | AdminStatus | ENUM | D
Index
A unique value for each caller number entry.
Filter
Caller number filter (leading) digits. Ignored if FilterType is set to 'anonymous'. Length: 0 to 24
FilterDescr
Description of this caller number filter. Length: 0 to 255
FilterType
Filter type of this caller number entry: normal: verify 'normal provided' numbers. anonymous: verify 'presentation not allowed' numbers. Enumerations: normal (1) anonymous (2)
Target
The caller number call can be distributed to an internal target: none: no target, reject the incoming call. group: a group of internal extensions. extension: one internal extension. announcement: direct routing to an announcement. Enumerations: none (0) group (1) extension (2) announcement (3)
TargetIndex
This variable contains index of the target table, if mpsCallerNumberTarget=group : index = mpsGroupIndex. mpsCallerNumberTarget=extension : index = mpsExtensionIndex. For all other target types this variable is ignored.
AnnFileDir
Name of directory (on flash medium) which contains file to be used for announcement. This variable references the entry in mpsWaveFile table where variable mpsWaveFileDirectory has identical content. This entry is only valid if variable mpsCallerNumberTarget is set to value announcement. Length: 0 to 255
AdminStatus
Just for MIB entry deletion. Enumerations: enabled (1) delete (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH