>> MIB - Management Information Base
>> Table: ospfAreaAggregateTable - (.1.3.6.1.2.1.14.14.1)
Description: A range of IP addresses specified by an IP address/IP network mask pair. For example, class B address range of X.X.X.X with a network mask of 255.255.0.0 includes all IP addresses from X.X.0.0 to X.X.255.255. Note that if ranges are range configured such that one range subsumes another range (e.g., 10.0.0.0 mask 255.0.0.0 and 10.1.0.0 mask 255.255.0.0), the most specific match is the preferred one.
ospfAreaAggregateTable
OID | Name | Type | Access
.1 | AreaId | IpAddress | RW
.2 | LsdbType | ENUM | RW
.3 | Net | IpAddress | RW
.4 | Mask | IpAddress | RW
.5 | Status | ENUM | D
.6 | Effect | ENUM | RW
AreaId
The Area the Address Aggregate is to be found within.
LsdbType
The type of the Address Aggregate. This field specifies the Lsdb type that this Address Ag- gregate applies to. Enumerations: summaryLink (3) nssaExternalLink (7)
Net
The IP Address of the Net or Subnet indicated by the range.
Mask
The Subnet Mask that pertains to the Net or Subnet.
Status
This variable displays the status of the en- try. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)
Effect
Subnets subsumed by ranges either trigger the advertisement of the indicated aggregate (ad- vertiseMatching), or result in the subnet's not being advertised at all outside the area. Enumerations: advertiseMatching (1) doNotAdvertiseMatching (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH