>> MIB - Management Information Base
>> Table: ospfNbrTable - (.1.3.6.1.2.1.14.10.1)
Description: The information regarding a single neighbor.
ospfNbrTable
OID | Name | Type | Access
.1 | IpAddr | IpAddress | R
.2 | AddressLessIndex | INTEGER | R
.3 | RtrId | IpAddress | R
.4 | Options | INTEGER | R
.5 | Priority | INTEGER | R
.6 | State | ENUM | R
.7 | Events | Counter | R
.8 | LsRetransQLen | Gauge | R
.9 | Status | ENUM | R
.10 | Permanence | ENUM | R
.11 | HelloSuppressed | ENUM | R
IpAddr
The IP address of this neighbor.
AddressLessIndex
On an interface having an IP Address, zero. On addressless interfaces, the corresponding value of ifIndex in the Internet Standard MIB. On row creation, this can be derived from the instance.
RtrId
A 32-bit integer (represented as a type IpAddress) uniquely identifying the neighboring router in the Autonomous System.
Options
A Bit Mask corresponding to the neighbor's options field. Bit 0, if set, indicates that the area accepts and operates on external information; if zero, it is a stub area. Bit 1, if set, indicates that the system will operate on Type of Service metrics other than TOS 0. If zero, the neighbor will ignore all metrics except the TOS 0 metric. Bit 2, if set, indicates that the system is ca- pable of routing IP Multicast datagrams; i.e., that it implements the Multicast Extensions to OSPF. Bit 3, if set, indicates that the associated area is an NSSA. These areas are capable of carrying type 7 external advertisements, which are translated into type 5 external advertise- ments at NSSA borders.
Priority
The priority of this neighbor in the designated router election algorithm. The value 0 signifies that the neighbor is not eligible to become the designated router on this particular network. Range: 0 to 255
State
The State of the relationship with this Neighbor. Enumerations: down (1) attempt (2) init (3) twoWay (4) exchangeStart (5) exchange (6) loading (7) full (8)
Events
The number of times this neighbor relationship has changed state, or an error has occurred.
LsRetransQLen
The current length of the retransmission queue.
Status
This variable displays the validity or invalidity of the entry. Setting it to 'invalid' has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent. Enumerations: valid (1) invalid (2)
Permanence
This variable displays the status of the en- try. 'dynamic' and 'permanent' refer to how the neighbor became known. Enumerations: dynamic (1) permanent (2)
HelloSuppressed
Indicates whether Hellos are being suppressed to the neighbor Enumerations: true (1) false (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH