>> MIB - Management Information Base
>> Table: wlanBridgeLinkStatsTable - (.1.3.6.1.4.1.272.4.46.33.1)
Description: Contains statistic information of the WLAN bridge link (WBL).
wlanBridgeLinkStatsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Address | MacAddress | R
.3 | State | ENUM | R
.4 | Signal | WlanRSSI | R
.5 | Noise | WlanRSSI | R
.6 | ConnectTime | Date | R
.7 | LastSeen | Date | R
.8 | TxBytes | Counter32 | R
.9 | RxBytes | Counter32 | R
.10 | TxRate | WlanRate | R
.11 | RxRate | WlanRate | R
.12 | RxFrames54 | Counter32 | R
.13 | RxFrames48 | Counter32 | R
.14 | RxFrames36 | Counter32 | R
.15 | RxFrames24 | Counter32 | R
.16 | RxFrames18 | Counter32 | R
.17 | RxFrames12 | Counter32 | R
.18 | RxFrames11 | Counter32 | R
.19 | RxFrames9 | Counter32 | R
.20 | RxFrames6 | Counter32 | R
.21 | RxFrames5 | Counter32 | R
.22 | RxFrames2 | Counter32 | R
.23 | RxFrames1 | Counter32 | R
.24 | TxFrames54 | Counter32 | R
.25 | TxFrames48 | Counter32 | R
.26 | TxFrames36 | Counter32 | R
.27 | TxFrames24 | Counter32 | R
.28 | TxFrames18 | Counter32 | R
.29 | TxFrames12 | Counter32 | R
.30 | TxFrames11 | Counter32 | R
.31 | TxFrames9 | Counter32 | R
.32 | TxFrames6 | Counter32 | R
.33 | TxFrames5 | Counter32 | R
.34 | TxFrames2 | Counter32 | R
.35 | TxFrames1 | Counter32 | R
.36 | RSSI1 | WlanRSSI | R
.37 | RSSI2 | WlanRSSI | R
.38 | RSSI3 | WlanRSSI | R
IfIndex
System generated unique WLAN bridge link index.
Address
Address where the WBL slave is associated with. Or on WBL master it is the MAC-Address of the connected WBL slave.
State
Show the current state of the WBL endpoint.
Signal
Received signal strength of latest received data frame.
Noise
This attribute shows the measured noise level in dBm, or 0 if no connection can be established.
ConnectTime
This attribute records the time at the moment the WBL endpoint successfully connect.
LastSeen
Timestamp of the last received frame by this WBL endpoint.
TxBytes
Total number of transmitted bytes.
RxBytes
Total number of received bytes.
TxRate
This attribute returns the data rate of the last successful transmitted packet in 500 Kbps units.
RxRate
This attribute returns the data rate of the last successful received packet in 500 Kbps units.
RxFrames54
This attribute shows the number of data frames that were received at 54 Mbps.
RxFrames48
This attribute shows the number of data frames that were received at 48 Mbps.
RxFrames36
This attribute shows the number of data frames that were received at 36 Mbps.
RxFrames24
This attribute shows the number of data frames that were received at 24 Mbps.
RxFrames18
This attribute shows the number of data frames that were received at 18 Mbps.
RxFrames12
This attribute shows the number of data frames that were received at 12 Mbps.
RxFrames11
This attribute shows the number of data frames that were received at 11 Mbps.
RxFrames9
This attribute shows the number of data frames that were received at 9 Mbps.
RxFrames6
This attribute shows the number of data frames that were received at 6 Mbps.
RxFrames5
This attribute shows the number of data frames that were received at 5.5 Mbps.
RxFrames2
This attribute shows the number of data frames that were received at 2 Mbps.
RxFrames1
This attribute shows the number of data frames that were received at 1 Mbps.
TxFrames54
This attribute shows the number of data frames that were transmitted at 54 Mbps.
TxFrames48
This attribute shows the number of data frames that were transmitted at 48 Mbps.
TxFrames36
This attribute shows the number of data frames that were transmitted at 36 Mbps.
TxFrames24
This attribute shows the number of data frames that were transmitted at 24 Mbps.
TxFrames18
This attribute shows the number of data frames that were transmitted at 18 Mbps.
TxFrames12
This attribute shows the number of data frames that were transmitted at 12 Mbps.
TxFrames11
This attribute shows the number of data frames that were transmitted at 11 Mbps.
TxFrames9
This attribute shows the number of data frames that were transmitted at 9 Mbps.
TxFrames6
This attribute shows the number of data frames that were transmitted at 6 Mbps.
TxFrames5
This attribute shows the number of data frames that were transmitted at 5.5 Mbps.
TxFrames2
This attribute shows the number of data frames that were transmitted at 2 Mbps.
TxFrames1
This attribute shows the number of data frames that were transmitted at 1 Mbps.
RSSI1
This attribute shows the received signal strength at the first receiver in dBm.
RSSI2
This attribute shows the received signal strength at the second receiver in dBm.
RSSI3
This attribute shows the received signal strength at the third receiver in dBm.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH