>> MIB - Management Information Base
>> Table: ipMRouteBoundaryTable - (.1.3.6.1.2.1.83.1.1.5.1)
Description: An entry (conceptual row) in the ipMRouteBoundaryTable representing a scoped boundary.
ipMRouteBoundaryTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | Address | IpAddress | R
.3 | AddressMask | IpAddress | R
.4 | Status | ENUM | D
IfIndex
The IfIndex value for the interface to which this boundary applies. Packets with a destination address in the associated address/mask range will not be forwarded out this interface. Range: 1 to 2147483647
Address
The group address which when combined with the corresponding value of ipMRouteBoundaryAddressMask identifies the group range for which the scoped boundary exists. Scoped addresses must come from the range 239.x.x.x as specified in RFC 2365.
AddressMask
The group address mask which when combined with the corresponding value of ipMRouteBoundaryAddress identifies the group range for which the scoped boundary exists.
Status
The status of this row, by which new entries may be created, or old entries deleted from this table. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH