>> MIB - Management Information Base
>> Table: voipSipProvExtTable - (.1.3.6.1.4.1.272.4.33.29.1)
Description: Describes additional information for a SIP provider account
voipSipProvExtTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | SendFromDisplay | ENUM | RW
.3 | SendFromUser | ENUM | RW
.4 | SendPPreferred | ENUM | RW
.5 | SendPAsserted | ENUM | RW
.6 | CLIPBilling | DisplayString | RW
Index
Unique table index of this entry. This value cannot be edited or changed. This value is identical to 'Index' number of parent entry in voipProviderTable or mpsTrunkGroupTable.
SendFromDisplay
Assignment of source information element to be used in SIP From header display for outgoing call. none: no display used username: the username, same as in Contact header clip: calling party number that should be shown on destination device clip-billing: calling party number for billing (must be a valid number) Enumerations: none (1) username (2) clip (3) clip-billing (4)
SendFromUser
Assignment of source information element to be used in SIP From header as username for outgoing call. For definition of values see voipSipProvExtSendFromDisplay. Enumerations: username (1) clip (2) clip-billing (3)
SendPPreferred
Assignment of source information element to be used in SIP P-Preferred-Identity header for outgoing call. For definition of values see voipSipProvExtSendFromDisplay. Enumerations: none (1) username (2) clip (3) clip-billing (4)
SendPAsserted
Assignment of source information element to be used in SIP P-Asserted-Identity header for outgoing call. For definition of values see voipSipProvExtSendFromDisplay. Enumerations: none (1) username (2) clip (3) clip-billing (4)
CLIPBilling
A valid phone number used if 'clip-billing' is selected. See above Length: 0 to 255

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH