>> MIB - Management Information Base
>> Table: localIcmpAllowTable - (.1.3.6.1.4.1.272.4.5.14.5.1)
Description: Filter rule table for incoming ICMP packets. o active rules have at least one of 'localIcmpAllowAddrMode' and 'localIcmpAllowIfMode' set to 'verify' o if there are active rules for a certain ICMP packet type, incoming packets of this type must match at least one of them. o incoming ICMP packets with a packet type not listed in any active rule are always allowed. o packets originating from 127.0.0.1 are always allowed
localIcmpAllowTable
OID | Name | Type | Access
.1 | AddrMode | ENUM | D
.2 | Addr | IpAddress | RW
.3 | Mask | IpAddress | RW
.4 | IfMode | ENUM | RW
.5 | IfIndex | INTEGER | RW
.6 | Type | ENUM | RW
AddrMode
Specifies wether or not the IP source address of incoming ICMP packets should checked Enumerations: dont-verify (1) verify (2) delete (3)
Addr
source IP address
Mask
source IP address mask
IfMode
Specifies wether or not the source interface of incoming ICMP packets should checked Enumerations: dont-verify (1) verify (2)
IfIndex
source interface index
Type
ICMP packet type Enumerations: echoRep (1) destUnreach (4) srcQuench (5) redirect (6) echo (9) timeExcds (12) parmProb (13) timestamp (14) timestampRep (15) addrMask (18) addrMaskRep (19)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH