>> MIB - Management Information Base
>> Table: wlanWDSAutoConfigTable - (.1.3.6.1.4.1.272.4.46.9.1)
Description: An entry in wlanWDSAutoConfigTable.
wlanWDSAutoConfigTable
OID | Name | Type | Access
.1 | LinkLockState | ENUM | RW
.2 | LinkConfigScanState | ENUM | RW
.99 | AutoConfigIfIndex | INTEGER | R
LinkLockState
This attribute defines if the bridge is locked. Lock state is common for all bridge links using the same radio. If the bridge is locked, it cannot be discovered by auto-configuration scan, and remote changing of any parameters is blocked. Enumerations: true (1) false (2)
LinkConfigScanState
This attribute defines the current auto-configuration state. idle(1) - In this state, writing scanning(2) starts an auto-configuration scan for bridge link peers. State will stay at scanning(2) while the scan is in progress. When the scan is finished, the results are available in the artemBidgePeersTable. scanning(2) - An auto-configuration scan for bridge link peers is currently in progress. When scanning has finished, the state will automatically change back to idle(1). busy(3) - An auto-configuration setup is currently in progress on this radio module. Writing this attribute in any state other than idle(1) is silently ignored. Enumerations: idle (1) scanning (2) busy (3)
AutoConfigIfIndex
Auxiliary index in wlanWDSAutoConfigTable.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH