>> MIB - Management Information Base
>> Table: mpsGroupTable - (.1.3.6.1.4.1.272.4.53.5.1.1)
Description: This table contains the information of the global team parameter for each extension group.
mpsGroupTable
OID | Name | Type | Access
.1 | Index | GroupIndex | RW
.2 | DisplayName | DisplayString | RW
.3 | Number | DisplayString | RW
.4 | NoReplyTimeout | INTEGER | RW
.5 | MulticastTrigger | INTEGER | RW
.6 | CallForwardingEnable | ENUM | RW
.7 | CallCalendar | Unsigned32 | RW
.8 | AdminStatus | ENUM | D
.9 | CallForwardingExtern | ENUM | RW
.10 | WrapUpTime | INTEGER | RW
.11 | ExtDescription | DisplayString | RW
.12 | Type | ENUM | RW
Index
A unique value for each group. Range: 1 to 100
DisplayName
Internal name of the group. Length: 0 to 20
Number
This variable contains the extension number of the group. Allowing all group members to be reached at all times for external and internal calls Length: 0 to 4
NoReplyTimeout
The linear and rotating team calls allow you to configure a time interval in seconds, after which the next member of the team will be called. Range: 1 to 999
MulticastTrigger
The linear and rotating team calls allow you to configure a time interval in seconds, after which all members of the team will be called in parallel. Range: 1 to 999
CallForwardingEnable
This value determine if call forwarding of the extension group member will be done(1) or not(2). Enumerations: true (1) false (2)
CallCalendar
Select a calendar to switch the call mode automatically. After you have selected a calendar you can set the active call mode. 0 (not active), 1 (day mode), 2 (night mode).
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
CallForwardingExtern
Use 2nd b-channel (false) or call deflection/partial rerouting (true) for call forwarding. Enumerations: true (1) false (2)
WrapUpTime
This variable contains the length of timer in seconds for the wrap up time. This timer value is used, if mpsGroupModeOperation is set to 'maxIdle'. Range: 0 to 999
ExtDescription
This value contains an extendend description in order to combine several mpsGroupTable entries in the GUI. Length: 0 to 20
Type
This variable contains the type of this group. The type is used to determine mpsGroupTables for different applications. Enumerations: standard (1) alarmInput (2)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH