>> MIB - Management Information Base
>> Table: mpsFaxSwitchModeTable - (.1.3.6.1.4.1.272.4.53.11.2.1)
Description: This table contains the information about fax switch modes.
mpsFaxSwitchModeTable
OID | Name | Type | Access
.1 | Index | FaxSwitchIndex | RW
.2 | Number | FaxSwitchModeIndex | RW
.3 | Extension | ExtensionIndexOrZero | RW
.4 | CNGTimeSlice | Unsigned32 | RW
.5 | RingingTime | Unsigned32 | RW
.6 | AdminStatus | ENUM | D
Index
A unique value for each fax switch. Use the same value in mpsFaxSwitchIndex and mpsFaxSwitchUserIndex as reference to this entry. Range: 1 to 65535
Number
A unique value or each mode of fax switch. The current active fax mode is set in mpsFaxSwitchUserModeNumber in mpsFaxSwitchUserTable. Range: 1 to 2
Extension
This variable contains the extension index of the fax port. Range: 0 to 65535
CNGTimeSlice
This variable contains the time slice in seconds to detect the CNG tone.
RingingTime
This variable contains the time in seconds how long the extension will be called.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) disable (2) delete (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH