>> MIB - Management Information Base
>> Table: mobileSmsTable - (.1.3.6.1.4.1.272.4.41.4.1.25.1)
Description: A single mobileSmsTable entry. Each entry is a copy of a SMS stored in the GSM/UMTS modem and/or on the SIM-Card used. Status information like 'received-unread', 'received-read', 'stored-unsent' and 'stored-sent' is additionally available. After being successfully sent an entry in the mobileSmsSendTable is moved to the mobileSmsTable. Since space in the GSM/UMTS modem and SIM-Card is limited applications have to delete entries from time to time.
mobileSmsTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | MsgStorage | ENUM | R
.3 | MsgSlot | INTEGER | R
.4 | MsgStatus | ENUM | D
.5 | ServiceCenterTimeStamp | DisplayString | R
.6 | ServiceCenterAddress | DisplayString | R
.7 | PhoneNumber | DisplayString | R
.8 | MsgFormat | ENUM | R
.9 | MsgCoding | ENUM | R
.10 | MsgData | OCTET STRING | R
IfIndex
The interface index of the mobile device which received the SMS or should transmit it.
MsgStorage
This object specifies the storage which holds the SMS. Available storages are: sm(1) -- SIM card storage me(2) -- Mobile Equipment storage mt(3) -- one of the ME associated storages bm(4) -- Broadcast Message storage ta(5) -- Terminal Adapter storage sr(6) -- Status Report storage Enumerations: sm (1) me (2) mt (3) bm (4) ta (5) sr (6)
MsgSlot
The actual index to address the SMS in 'mobileSmsMsgStorage'. Range: 0 to 65535
MsgStatus
The status of the SMS. The first four states correspond with 3GPP TS27.005. For incoming SMS the Status is set to `rec-unread(1)'. After reading the SMS the Status is set to `rec-read(2)'. On storing one SMS for sending the Status is `sto-unsent(3)'. If SMS was sent successfully Status changes to `sto-sent(4)'. In order to delete the SMS permanently set Status to `delete(5)'. This object can only be set to `delete'. Other settings are ignored silently. Enumerations: rec-unread (1) rec-read (2) sto-unsent (3) sto-sent (4) delete (5)
ServiceCenterTimeStamp
The date/time the SMS is sent or received. Length: 0 to 64
ServiceCenterAddress
The Service Center Address used to send or receive this SMS. Length: 0 to 64
PhoneNumber
The origination or destination address of this SMS depending on the value of 'mobileSmsMsgStatus'. Length: 0 to 64
MsgFormat
The message format of the SMS. Traditional SMS use plain `txt(2)' format. Special or Unicode SMS use `pdu(1)' format. Enumerations: pdu (1) txt (2)
MsgCoding
This object specifies the coding of the SMS user data section. Enumerations: ira (1) gsm (2) ucs2 (3) pc437 (4) iso8859-1 (5) uh-7bit (6) uh-8bit (7)
MsgData
The raw data of the complete SMS. Length: 0 to 160

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH