>> MIB - Management Information Base
>> Table: wlcVSSStatTable - (.1.3.6.1.4.1.272.4.61.1.26.1)
Description: This table contains statistic information about each VSS.
wlcVSSStatTable
OID | Name | Type | Access
.1 | VSSIndex | INTEGER | R
.2 | Current | INTEGER | R
.3 | BytesTx | Counter32 | R
.4 | BytesRx | Counter32 | R
.5 | BSSID | MacAddress | R
.6 | OperState | ENUM | R
.7 | SoftTotalDenied | INTEGER | R
.8 | BSMovements | INTEGER | R
.9 | ClearCounter | ENUM | RW
.10 | TotalDenied | INTEGER | R
.11 | RSSIThresholdPurges | INTEGER | R
VSSIndex
The unique VSS index.
Current
Number of currently associated stations.
BytesTx
Transmitted Bytes.
BytesRx
Received Bytes.
BSSID
This object contains the current BSSID for the service set. Length: 6 to 6
OperState
This object contains the current OperState for the service set. Enumerations: true (1) false (2)
SoftTotalDenied
Number of rejected clients due to wlcVSSProfileSoftTotal limit.
BSMovements
Number of clients moved to other band by band steering mechanism.
ClearCounter
counting := accounting is active, clearing := clear all statistics Enumerations: counting (1) clearing (2)
TotalDenied
Number of rejected clients due to wlcVSSProfileTotal limit.
RSSIThresholdPurges
Number of dissociated clients due to low RSSI.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH