>> MIB - Management Information Base
>> Table: hdsl2ShdslEndpointConfTable - (.1.3.6.1.4.1.272.4.35.1.1.4.1)
Description: An entry in the hdsl2ShdslEndpointConfTable. Each entry represents a single segment endpoint in a HDSL2/SHDSL line. It is indexed by the ifIndex of the HDSL2/SHDSL line.
hdsl2ShdslEndpointConfTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Side | ENUM | RW
.5 | WireInterface | ENUM | RW
.6 | MinLineRate | INTEGER | RW
.7 | MaxLineRate | INTEGER | RW
.8 | TransmissionMode | ENUM | RW
.10 | CurrCondTargetMarginDown | INTEGER | RW
.11 | WorstCaseTargetMarginDown | INTEGER | RW
.12 | CurrCondTargetMarginUp | INTEGER | RW
.13 | WorstCaseTargetMarginUp | INTEGER | RW
.14 | GroupId | INTEGER | RW
.15 | LineProbeEnable | ENUM | RW
.16 | LicenseUsage | ENUM | R
.17 | PamMode | INTEGER | RW
.18 | TotalMinLineRate | INTEGER | RW
.19 | MinWirePairs | INTEGER | RW
.20 | CapListStyle | ENUM | RW
.21 | UsedTargetMargins | BITS | RW
IfIndex
This object specifies the associated interface index of this HDSL2/SHDSL line.
Side
The side of the unit associated with this segment endpoint - Network/Customer side - as per the Hdsl2ShdslUnitSide textual convention. Enumerations: networkSide (1) customerSide (2)
WireInterface
This object configures the bonding mode of the SHDSL Line. twoWire(1) : no bonding is used fourWire(2) : four-wire mode fourWireStandard(3) : four-wire mode, disable globespan enhanced mode fourWireIMA(4) : 2 wire pairs bonded with IMA sixWire(5) : 3 wire pairs in m-pair mode sixWireIMA(6) : 3 wire pairs bonded with IMA eightWire(7) : 4 wire pairs in m-pair mode eightWireIMA(8) : 4 wire pairs bonded with IMA not-used(9) : wire pair inactive groupMember(10) : wire pair belongs to a bonding group twoWireEFM(11) : 2 wire EFM mode fourWireEFM(12) : 2 wire pairs in EFM mode with PAF bonding sixWireEFM(13) : 3 wire pairs in EFM mode with PAF bonding eightWireEFM(14) : 4 wire pairs in EFM mode with PAF bonding Enumerations: twoWire (1) fourWire (2) fourWireStandard (3) fourWireIMA (4) sixWire (5) sixWireIMA (6) eightWire (7) eightWireIMA (8) not-used (9) groupMember (10) twoWireEFM (11) fourWireEFM (12) sixWireEFM (13) eightWireEFM (14)
MinLineRate
This object configures the minimum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
MaxLineRate
This object configures the maximum transmission rate for the associated SHDSL Line in bits-per-second (bps). If the minimum line rate equals the maximum line rate (hdsl2ShdslSpanMaxLineRate), the line rate is considered 'fixed'. If the minimum line rate is less than the maximum line rate, the line rate is considered 'rate-adaptive'. Range: 0 to 22784000
TransmissionMode
This object specifies the regional setting for the SHDSL line: region1 - ITU-T G.991.2 Annex A region2 - ITU-T G.991.2 Annex B Enumerations: region1 (1) region2 (2) region1or2 (3)
CurrCondTargetMarginDown
This object specifies the downstream current condition target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 21
WorstCaseTargetMarginDown
This object specifies the downstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 65535
CurrCondTargetMarginUp
This object specifies the upstream current condition target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 21
WorstCaseTargetMarginUp
This object specifies the upstream worst case target SNR margin for a SHDSL line. The SNR margin is the difference between the desired SNR and the actual SNR. Target SNR margin is the desired SNR margin for a unit. Range: -10 to 21
GroupId
This object defines which wire-pairs belong to the same M-pair group or IMA group. Members of the same group have the same entry. Range: 0 to 255
LineProbeEnable
This object specifies the configuration of the PMMS behavior: auto - Line Probe is enabled if hdsl2ShdslEndpointConfMinLineRate < hdsl2ShdslEndpointConfMaxLineRate. disable - Line Probe is disabled. enable - Line Probe is enabled. enable_std - Line Probe is enabled and standard compliant behaviour is enforced. Enumerations: auto (1) disable (2) enable (3) enable-std (4)
LicenseUsage
Shows which license type is currently used for this SHDSL interface. Enumerations: none (1) missing (2) shdsl (3)
PamMode
This object specifies which modulation modes are allowed for this wire pair. 16 - 16-TCPAM, used for Annex A,B and F,G. 32 - 32-TCPAM, used for Annex F,G only. 4, 8, 64, 128 - non standard proprietary modes. On CPE site more than one mode can be allowed by adding the values. On CO site only the highest mode is used if several values are added. Range: 4 to 252
TotalMinLineRate
This object configures the minimum transmission rate in bits-per-second (bps) for the associated SHDSL bundle. The associated interfaces go up only when the sum of the data rates of the associated wire pairs in state Showtime reaches or exceeds the specified value. This variable has no effect with single pair modes. Range: 1 to 50000000
MinWirePairs
This object configures the minimum number of wire pairs for the associated SHDSL bundle. The associated interfaces go up only when at least the specified number of wire pairs is connected and in Showtime. This variable has no effect with single pair modes. Range: 1 to 4
CapListStyle
This object specifies the data format of the capability list, that is exchanged during the G.994.1 handshake: auto - automatic detection of the used capability list style. old - only ATM modes till 2312 kbps can be negotiated. new - all modes can be negotiated. Enumerations: auto (1) old (2) new (3)
UsedTargetMargins
Contains indicates whether a target SNR margin is enabled or disabled. This is a bit-map of possible settings. The various bit positions are: currCondDown current condition downstream target SNR margin enabled worstCaseDown worst case downstream target SNR margin enabled currCondUp current condition upstream target SNR margin enabled worstCaseUp worst case upstream target SNR margin enabled. Enumerations: currCondDown (0) worstCaseDown (1) currCondUp (2) worstCaseUp (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH