>> MIB - Management Information Base
>> Table: ipDnsServerOperTable - (.1.3.6.1.4.1.272.4.5.20.33.1)
Description: Contains one operational version for each parent-entry in ipDnsServerCfgTable.
ipDnsServerOperTable
OID | Name | Type | Access
.1 | ParentIndex | INTEGER | R
.2 | OperStatus | ENUM | R
.3 | Mode | ENUM | R
.4 | Priority | INTEGER | R
.5 | PrimaryAddress | IpAddress | R
.6 | SecondaryAddress | IpAddress | R
.7 | IfIndex | INTEGER | R
.8 | NumRequests | INTEGER | R
.9 | NumPosReplies | INTEGER | R
.10 | NumNegReplies | INTEGER | R
.11 | Ip6PrimaryAddress | InetAddressIPv6 | R
.12 | Ip6SecondaryAddress | InetAddressIPv6 | R
.13 | IpVersion | ENUM | R
ParentIndex
Copied from ipDnsServerCfgIndex of parent-entry.
OperStatus
Operation-status of this entry, depending on ipDnsServerCfgAdminStatus of parent-entry and on ifOperStatus if ipDnsServerOperIfIndex specified. Enumerations: enabled (1) disabled (2) dormant (3)
Mode
Copied from ipDnsServerCfgMode of parent-entry. Enumerations: manual (1) automatic (2)
Priority
Copied from ipDnsServerCfgPriority of parent-entry. Range: 0 to 9
PrimaryAddress
In manual case, copied frome ipDnsServerCfgPrimaryAddress of parent-entry. In automatic case, initialised to 0 and updated via DHCP/IPCP.
SecondaryAddress
In manual case, copied frome ipDnsServerCfgSecondaryAddress of parent-entry. In automatic case, initialised to 0 and updated via DHCP/IPCP.
IfIndex
Copied from ipDnsServerCfgIfIndex of parent-entry.
NumRequests
Number of sent requests.
NumPosReplies
Number of received positive replies.
NumNegReplies
Number of received negative replies.
Ip6PrimaryAddress
The primary DNS Server IPv6 Address.
Ip6SecondaryAddress
The secondary DNS Server IPv6 Address.
IpVersion
Determines whether the IPv4 or IPv6 DNS Server address pair should be considered.

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH