>> MIB - Management Information Base
>> Table: wlcAutoSelectorTable - (.1.3.6.1.4.1.272.4.61.1.35.1)
Description: The table defines a selector to lookup a WTP in the wlcAutoWTPTable. See wlcAutoWTPSelectorIndex.
wlcAutoSelectorTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | MacAddress | MacAddress | RW
.3 | InetAddressType | ENUM | RW
.4 | InetAddress | IpAddress | RW
.5 | InetMask | IpAddress | RW
.6 | AdminStatus | ENUM | D
Index
Unique selector index.
MacAddress
Selector: ethernet MAC address of the WTP. The address 00:00:00:00:00:00 matches for any MAC address. Length: 6 to 6
InetAddressType
Selector: IP address type. It may be one of: -unknown(0): means that any IP address matches -ipv4(1) : an IPv4 address -ipv6(2) : an IPv6 address All other values are not supported and treated like unknown. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
InetAddress
Selector: IP address.
InetMask
Selector: IP netmask.
AdminStatus
Delete the requested selector. Enumerations: enabled (1) disabled (2) delete (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH