>> MIB - Management Information Base
>> Table: wlcScanResultsTable - (.1.3.6.1.4.1.272.4.61.1.27.1)
Description: This table contains the list of BSS entries found by foreground or background scanning.
wlcScanResultsTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | wlanIfIndex | INTEGER | R
.3 | BSSID | MacAddress | R
.4 | RSSI | WlanRSSI | R
.5 | SSID | DisplayString | R
.6 | Channel | INTEGER | R
.7 | Privacy | ENUM | R
.8 | Type | ENUM | R
.9 | WPAUnicastCipher | BITS | R
.10 | RSNUnicastCipher | BITS | R
.11 | APType | ENUM | R
.12 | LastSeen | Date | R
.13 | Bandwidth | ENUM | R
.14 | FirstChannel0 | INTEGER | R
.15 | FirstChannel1 | INTEGER | R
.16 | Mode | ENUM | R
.17 | Rates | DisplayString | R
.18 | BSSColor | INTEGER | R
.19 | Fingerprint | OCTET STRING | R
Index
Auxiliary index for different BSS entries.
wlanIfIndex
Index of WLAN Interface the scan results belong to.
BSSID
BSSID of this BSS. Length: 6 to 6
RSSI
Receive signal strength of this BSS. Range: -110 to 0
SSID
SSID aka network name of this BSS. If broadcasting of SSID is disabled on this BSS, this string may be empty. Length: 0 to 255
Channel
The channel where this BSS send its beacons on.
Privacy
This attribute contains the privacy type of the scanned device. Enumerations: none (1) wep (2) wpa-psk (3) wpaandwpa2-psk (4) wpa2-psk (5) wpa-enterprise (6) wpaandwpa2-enterprise (7) wpa2-enterprise (8) wpa2andwpa3-psk (9) wpa3-psk (10) wpa2andwpa3-enterprise (11) wpa3-enterprise (12) owe (13) owe-transition (14) cnsa (15)
Type
This attribute contains the device type of the scanned device. Enumerations: access-point (1) ad-hoc (2) mesh (3)
WPAUnicastCipher
This attribute contains the WPA unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4) cipher-aes-ccmp-256 (5) cipher-aes-gcmp-128 (6) cipher-aes-gcmp-256 (7)
RSNUnicastCipher
This attribute contains the RSN unicast ciphers of the scanned device. Enumerations: cipher-none (0) cipher-wep40 (1) cipher-wep104 (2) cipher-tkip (3) cipher-aes (4) cipher-aes-ccmp-256 (5) cipher-aes-gcmp-128 (6) cipher-aes-gcmp-256 (7)
APType
This attribute contains the type of the scanned access point. 'own' -> managed AP, 'neighborhood' -> neighborhood AP 'rogue' -> foreign AP but with one of our SSIDs, 'own-manipulated' -> managed AP but with manipulated configuration. 'knownneighbor' -> a neigborhood AP but well known by wlcKnownAPTable 'knownrogue' -> foreign AP with one of our SSIDs but is well known by wlcKnownAPTable Enumerations: own (1) neighborhood (2) rogue (3) own-manipulated (4) knownneighbor (5) knownrogue (6)
LastSeen
This attribute contains that time when an access point or client was seen for the last time. Range: 0 to -1
Bandwidth
Used bandwidth of this BSS. Enumerations: b20MHz (1) b40MHz (2) b80MHz (3) b80MHzand80MHz (4) b160MHz (5)
FirstChannel0
First channel in ieee notation of the first band. Range: 1 to 256
FirstChannel1
First channel in ieee notation of the second band. This is used on 80MHz+80MHz in .11ac mode. Value 0, if this field is not used. Range: 0 to 256
Mode
Used mode of this BSS. Enumerations: unknown (1) m802-11a (2) m802-11b (3) m802-11g (4) m802-11n (5) m802-11ac (6) m802-11ax (7)
Rates
Announced rates of the scanned device. When a rate is marked as basic rate, the letter B will be shown after the rate. Length: 0 to 255
BSSColor
Numerical identifier of the BSS used by 802.11ax capable radios to differentiate networks. Note that the value 0 is set when no color is present. Range: 0 to 63
Fingerprint
Fingerprint which is equal for BSS, which presumably were emitted by the same neighbor AP radio. Thus the fingerprint helps determining which neighbor BSS belong to the same AP device and the true number of physical neighbor APs. It is computed from wlcScanResultsChannel, wlcScanResultsBandwidth, wlcScanResultsFirstChannel0 and wlcScanResultsBSSID. Length: 8 to 8

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH