>> MIB - Management Information Base
>> Table: ipDns - (.1.3.6.1.4.1.272.4.5.20)
ipDns
OID | Name | Type | Access
.1 | DhcpAssign | ENUM | RW
.2 | IpcpAssign | ENUM | RW
.3 | UsePosCache | ENUM | RW
.4 | UseNegCache | ENUM | RW
.5 | MaxCacheSize | INTEGER | RW
.6 | PositiveTtl | INTEGER | RW
.7 | NegativeTtl | INTEGER | RW
.8 | DefaultIfIndex | INTEGER | RW
.9 | NumReceives | INTEGER | R
.10 | NumInvalids | INTEGER | R
.11 | NumRequests | INTEGER | R
.12 | NumCacheHits | INTEGER | R
.13 | NumForwards | INTEGER | R
.14 | NumOks | INTEGER | R
.15 | NumFails | INTEGER | R
.17 | DynamicGlobals | ENUM | RW
.20 | CheckBailiwick | ENUM | RW
DhcpAssign
Assignment policy when a BinTec router acts as a DHCP-server and is asked for nameserver addresses. Possible values: - none: Do not send any nameserver-addresses. - self: Send own address as the only nameserver. - global: Send addresses from global nameserver-table. Enumerations: none (1) self (2) global (3)
IpcpAssign
Assignment policy when a BinTec router is asked for nameservers during IPCP negotiation. Possible values: - none: Do not send any nameserver addresses. - self: Send own address as the only nameserver. - global: Send addresses from global namerserver-table. Enumerations: none (1) self (2) global (3)
UsePosCache
Decides whether positive dynamic caching is done or not. Enumerations: no (1) yes (2)
UseNegCache
Decides whether negative dynamic caching is done or not. Enumerations: no (1) yes (2)
MaxCacheSize
Defines maximum number of dynamic DNS-table-entries. If this limit is reached, the least recently used dynamic entry is discarded if a new one is to be added.
PositiveTtl
Time-to-live in seconds reported for positive static entries.
NegativeTtl
Time-to-live in seconds reported for negative static entries, and initial time-to-live for negative dynamic cache-entries.
DefaultIfIndex
Interface-index (if not -1) of DHCP/IPCP-assigned nameserver that should be used as fallback for DNS-forwarding if not found by other mechanism (e.g. manually configured global nameserver or address/interface specified by application or wildcard-domain-forwarding-entry).
NumReceives
The number of packets received.
NumInvalids
The number of invalid packets received.
NumRequests
The number of questions received. If a packet is received, this variable is incremented by the number of question records contained in the packet.
NumCacheHits
The number of times a question could be answered immediately due to a cache entry.
NumForwards
The number of questions forwarded to other nameservers.
NumOks
The number of requests answered successfully.
NumFails
The number of requests answered with a SERVFAIL packet.
DynamicGlobals
Determines if 'automatic' entries (see ipDnsServerCfgMode) are stored in global nameserver-table: - yes: Make 'automatic' nameserver-entries. - no: Do NOT make 'automatic' nameserver-entries. Enumerations: yes (1) no (2)
CheckBailiwick
Determines if 'Bailiwick' check of answer, authority and additional records should be performed or not. If set to webfilter(3) special policies defined otherwise will be used. Enumerations: yes (1) no (2) webfilter (3)

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH