>> MIB - Management Information Base
>> Table: wlcVSSProfileExtTable - (.1.3.6.1.4.1.272.4.61.1.42.1)
Description: Extended WLC VSS profile table.
wlcVSSProfileExtTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Dot11K | ENUM | RW
.3 | Dot11V | ENUM | RW
.4 | Dot11R | ENUM | RW
.5 | radiusSrvIndex | INTEGER | RW
Index
Unique VSS profile ext index. Note that each row of this table has an equivalent at the wlcVSSProfileTable so adding/deleting operations must be done there.
Dot11K
Provides information to discover the best available AP of the network topology Enumerations: disabled (1) enabled (2)
Dot11V
Allows the wireless client devices to exchange information about the network topology Enumerations: disabled (1) enabled (2)
Dot11R
Behavior of the fast BSS transition (FT) or fast roaming on this interface Enumerations: disabled (1) over-the-air (2) over-the-ds (3)
radiusSrvIndex
Optional VSS-specific wlcRadiusSrvIndex for overriding default wlcWTPradiusSrvIndex, else 0

MIB Reference to Software Version 10.2.12 generated on 2023/08/29. Provided by webmaster@bintec-elmeg.com Copyright ©2023 by bintec elmeg GmbH